{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":37,"rows_kept":6,"merged":[[0,14,0,16]],"flags":["formulas_cached_only"]}
["备注","序号","工段/部门","位号","仪表名称","测点","介质","设计温度/℃","进口压力/Mpa","操作粘度/cp","操作密度/kg/m3","管径","建议量程","最大允许压降/KPa","最小/正常/最大流量",null,null,"单位","是否配置过滤器","信号输出","现场显示","供电要求","接线制","电气接口","流量精度要求/%","密度精度要求/kg/m3","是否带二次表","接液材质","过程连接形式","法兰标准及压力等级","法兰尺寸","防爆/防护等级","是否夹套伴热","数量/个/台","申购日期","生产厂家","备注"]
[null,1,"罐区","FI-LAO309","质量流量计","4号位成品甲酯发货流量","油脂",50,0.3,5,880,125,"/",80,10,77,100,"t/h","否","2路4-20mA+HART","背光LCD","DC24V","2+4线制","M20*1.5","≤0.3（数值）",2,"/","316L","法兰连接","HG20592-09,PN16",null,"非防爆/IP65","否",1,"2022/09/21"]
[null,2,"罐区","FI-LAO311","质量流量计","5号位成品甲酯发货流量","油脂",50,0.3,5,880,125,"/",80,10,77,100,"t/h","否","2路4-20mA+HART","背光LCD","DC24V","2+4线制","M20*1.5","≤0.3（数值）",2,"/","316L","法兰连接","HG20592-09,PN16",null,"非防爆/IP65","否",1,"2022/09/21"]
[null,3,"罐区","FI-LAO308","质量流量计","6号位成品甲酯发货流量","油脂",50,0.3,5,880,125,"/",80,10,77,100,"t/h","否","2路4-20mA+HART","背光LCD","DC24V","2+4线制","M20*1.5","≤0.3（数值）",2,"/","316L","法兰连接","HG20592-09,PN16",null,"非防爆/IP65","否",1,"2022/09/21"]
[null,4,"罐区","FI-LAO301","质量流量计","9号位成品发货流量1","植物沥青",80,0.3,500,930,150,"/",80,10,77,100,"t/h","否","2路4-20mA+HART","背光LCD","DC24V","2+4线制","M20*1.5","≤0.3（数值）",2,"/","316L","法兰连接","HG20592-09,PN16",null,"非防爆/IP65","否",1,"2022/09/21"]
[null,5,"罐区","FI-LAO302","质量流量计","9号位成品发货流量2","油脂",50,0.3,5,880,125,"/",80,10,77,100,"t/h","否","2路4-20mA+HART","背光LCD","DC24V","2+4线制","M20*1.5","≤0.3（数值）",2,"/","316L","法兰连接","HG20592-09,PN16",null,"非防爆/IP65","否",1,"2022/09/21"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}