{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":5,"rows_kept":3,"merged":[[0,0,2,0],[0,4,1,4]],"flags":["formulas_cached_only"]}
["手动重型球阀\n（实心球）","碳钢","DN50  PN16 介质温度：150度，水油蒸汽",20,"仓库备件"]
[null,"316L","DN50  PN16 介质温度：150度，水油蒸汽",5]
[null,304,"DN200 PN16 介质温度：长期300度  油脂",1]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}