{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":2,"n_cols":9,"rows_kept":2,"flags":["formulas_cached_only"]}
["名称","材质","口径","插深","介质","工作温度","绝压","隔爆","数量"]
["音叉液位开关","316L","DN50","400MM","植物沥青","250度","1Kpa","EXdIIBT2","2台"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}