{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","各个型号数量","Sheet2"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":253,"n_cols":10,"rows_kept":253,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[1,6,1,11]]}
["序号","名称","描述","单位","工程量","备注"]
[{"$nulls":6},"软密封球阀均采用防火防静电结构，球阀均为实心球"]
[117,"截止阀,DN50,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",1,"J41Y-16C DN50",null,null,"球阀种类","7种"]
[118,"截止阀,DN80,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",3,"J41Y-16C DN80",null,null,"截止阀种类","5种"]
[119,"截止阀,DN150,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",1,"J41Y-16C DN150",null,null,"止回阀","16种"]
[120,"截止阀,DN25,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",32,"J41Y-16C DN25",null,null,"蝶阀种类","4种"]
[121,"球阀,DN20,PN16,RF,Floating Ball","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",10,"Q41F-16C DN20",null,null,"闸阀","2种"]
[122,"球阀,DN25,PN16,RF,Floating Ball","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",5,"Q41F-16C DN25",null,null,"Y型过滤器","2种"]
[123,"止回阀,DN350,PN16,RF,Dual Plate, Wafer,双板止回阀应水平安装，铰链销垂直，或垂直安装，流向向上","JB/T8937,阀体:WCB 阀芯:13Cr","个",5,"H76H-16C DN350"]
[124,"蝶阀,DN350,PN16,RF,Wafer, Gear","GB/T12238,阀体:WCB 阀芯:13Cr/EPDM","个",10,"D371X-16C DN350"]
[397,"闸阀,DN50,PN16,RF,BB, OS&Y","GB/T12234,阀体:WCB 阀芯:13Cr/STL","个",7,"Z41Y-16C DN50"]
[398,"闸阀,DN65,PN16,RF,BB, OS&Y","GB/T12234,阀体:WCB 阀芯:13Cr/STL","个",8,"Z41Y-16C DN65"]
[399,"闸阀,DN200,PN16,RF,BB, OS&Y","GB/T12234,阀体:WCB 阀芯:13Cr/STL","个",1,"Z41Y-16C DN200"]
[400,"闸阀,DN20,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",56,"Z41Y-16C DN20"]
[401,"闸阀,DN25,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",1,"Z41Y-16C DN25"]
[402,"闸阀,DN32,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",1,"Z41Y-16C DN32"]
[403,"截止阀,DN50,PN16,RF,BB, OS&Y","GB/T12235,阀体:CF8 阀芯:304","个",1,"J41W-16P DN50"]
[404,"截止阀,DN65,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","GB/T12235,阀体:CF8 阀芯:304/STL","个",2,"J41Y-16P DN65"]
[405,"截止阀,DN50,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr","个",34,"J41H-16C DN50"]
[406,"截止阀,DN65,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr","个",12,"J41H-16C DN65"]
[407,"截止阀,DN125,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr","个",4,"J41H-16C DN125"]
[408,"截止阀,DN150,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr","个",4,"J41H-16C DN150"]
[409,"截止阀,DN50,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",92,"J41Y-16C DN50"]
[410,"截止阀,DN50,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",2,"J41Y-16C DN50"]
[411,"截止阀,DN80,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",12,"J41Y-16C DN80"]
[412,"截止阀,DN150,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",2,"J41Y-16C DN150"]
[413,"截止阀,DN25,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr","个",30,"J41H-16C DN25"]
[414,"截止阀,DN32,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr","个",10,"J41H-16C DN32"]
[415,"截止阀,DN20,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",64,"J41Y-16C DN20"]
[416,"截止阀,DN25,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",44,"J41Y-16C DN25"]
[417,"截止阀,DN32,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",88,"J41Y-16C DN32"]
[418,"截止阀,DN40,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",8,"J41Y-16C DN40"]
[419,"球阀,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:CF3M 阀芯:316L/PTFE","个",2,"Q41F-16RL DN20"]
[420,"球阀,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:CF3M 阀芯:316L/PTFE","个",1,"Q41F-16RL DN25"]
[421,"球阀,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:CF3M 阀芯:316L/PTFE","个",4,"Q41F-16RL DN80"]
[422,"球阀,DN20,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",63,"Q41F-16P DN20"]
[423,"球阀加长阀杆,DN20,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",15,"Q41F-16P DN20"]
[424,"球阀加长阀杆,DN25,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",24,"Q41F-16P DN25"]
[425,"球阀加长阀杆,DN50,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",7,"Q41F-16P DN50"]
[426,"球阀加长阀杆,DN65,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",2,"Q41F-16P DN65"]
[427,"球阀加长阀杆,DN80,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",1,"Q41F-16P DN80"]
[428,"球阀加长阀杆,DN100,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",1,"Q41F-16P DN100"]
[429,"球阀,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",18,"Q41Y-16P DN20"]
[430,"球阀加长阀杆,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",30,"Q41Y-16P DN20"]
[431,"球阀,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",21,"Q41Y-16P DN25"]
[432,"球阀加长阀杆,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",58,"Q41Y-16P DN25"]
[433,"球阀加长阀杆,DN32,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",6,"Q41Y-16P DN32"]
[434,"球阀,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",6,"Q41Y-16P DN50"]
[435,"球阀加长阀杆,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",38,"Q41Y-16P DN50"]
[436,"球阀加长阀杆,DN65,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",50,"Q41Y-16P DN65"]
[437,"球阀,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",2,"Q41Y-16P DN80"]
[438,"球阀加长阀杆,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",10,"Q41Y-16P DN80"]
[439,"球阀,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",4,"Q41Y-16P DN100"]
[440,"球阀加长阀杆,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",37,"Q41Y-16P DN100"]
[441,"球阀,DN20,PN16,RF,Floating Ball","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",32,"Q41F-16C DN20"]
[442,"球阀,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",79,"Q41F-16C DN20"]
[443,"球阀加长阀杆,DN20,PN16,RF,Floating Ball","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",8,"Q41F-16C DN20"]
[444,"球阀加长阀杆,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",49,"Q41F-16C DN20"]
[445,"球阀,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",151,"Q41F-16C DN25"]
[446,"球阀加长阀杆,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",30,"Q41F-16C DN32"]
[447,"球阀,DN32,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",20,"Q41F-16C DN32"]
[448,"球阀加长阀杆,DN32,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",6,"Q41F-16C DN32"]
[449,"球阀,DN40,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",2,"Q41F-16C DN40"]
[450,"球阀,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",63,"Q41F-16C DN50"]
[451,"球阀加长阀杆,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",40,"Q41F-16C DN50"]
[452,"球阀,DN65,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",32,"Q41F-16C DN65"]
[453,"球阀加长阀杆,DN65,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",46,"Q41F-16C DN65"]
[454,"球阀,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",8,"Q41F-16C DN80"]
[455,"球阀加长阀杆,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",48,"Q41F-16C DN80"]
[456,"球阀,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",5,"Q41F-16C DN100"]
[457,"球阀加长阀杆,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",8,"Q41F-16C DN100"]
[458,"球阀,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",4,"Q41Y-16C DN20"]
[459,"球阀加长阀杆,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",36,"Q41Y-16C DN20"]
[460,"球阀,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",8,"Q41Y-16C DN25"]
[461,"球阀加长阀杆,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",21,"Q41Y-16C DN25"]
[462,"球阀,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",4,"Q41Y-16C DN50"]
[463,"球阀加长阀杆,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",10,"Q41Y-16C DN50"]
[464,"球阀加长阀杆,DN65,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",34,"Q41Y-16C DN65"]
[465,"球阀,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",4,"Q41Y-16C DN80"]
[466,"球阀加长阀杆,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",24,"Q41Y-16C DN80"]
[467,"球阀加长阀杆,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",10,"Q41Y-16C DN100"]
[468,"球阀,DN20,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",7,"Q41F46-16C DN20"]
[469,"球阀加长阀杆,DN20,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",8,"Q41F46-16C DN20"]
[470,"球阀,DN25,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",21,"Q41F46-16C DN25"]
[471,"球阀加长阀杆,DN25,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",86,"Q41F46-16C DN25"]
[472,"球阀,DN50,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",5,"Q41F46-16C DN50"]
[473,"球阀加长阀杆,DN50,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",107,"Q41F46-16C DN50"]
[474,"球阀,DN65,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",10,"Q41F46-16C DN65"]
[475,"球阀加长阀杆,DN65,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",27,"Q41F46-16C DN65"]
[476,"球阀,DN80,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",15,"Q41F46-16C DN80"]
[477,"球阀加长阀杆,DN80,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",12,"Q41F46-16C DN80"]
[478,"球阀,DN100,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",1,"Q41F46-16C DN100"]
[479,"球阀加长阀杆,DN100,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",64,"Q41F46-16C DN100"]
[480,"止回阀,DN80,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF3M 阀芯:316L/STL","个",1,"H44Y-16RL DN80"]
[481,"止回阀,DN50,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304","个",2,"H44W-16P DN50"]
[482,"止回阀,DN50,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304/STL","个",4,"H44Y-16P DN50"]
[483,"止回阀,DN65,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304/STL","个",2,"H44Y-16P DN65"]
[484,"止回阀,DN50,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:WCB 阀芯:13Cr","个",10,"H44H-16C DN50"]
[485,"止回阀,DN65,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:WCB 阀芯:13Cr","个",22,"H44H-16C DN65"]
[486,"止回阀,DN80,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:WCB 阀芯:13Cr","个",9,"H44H-16C DN80"]
[487,"止回阀,DN125,PN16,RF,Swing, Lined,旋启式止回阀应水平安装，阀板开启朝上，或垂直安装，流向向上","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",8,"H44F46-16C DN125"]
[488,"止回阀,DN25,PN16,RF,Ball / Lift, Lined,球型升降式式止回阀应垂直安装，流向向上","HG/T3704,阀体:WCB / PTFE Liner 阀芯:PTFE","个",6,"HQ41F46-16C DN25"]
[489,"止回阀,DN50,PN16,RF,Ball / Lift, Lined,球型升降式式止回阀应垂直安装，流向向上","HG/T3704,阀体:WCB / PTFE Liner 阀芯:PTFE","个",19,"HQ41F46-16C DN50"]
[490,"止回阀,DN65,PN16,RF,Ball / Lift, Lined,球型升降式式止回阀应垂直安装，流向向上","HG/T3704,阀体:WCB / PTFE Liner 阀芯:PTFE","个",9,"HQ41F46-16C DN65"]
[491,"止回阀,DN100,PN16,RF,Ball / Lift, Lined,球型升降式式止回阀应垂直安装，流向向上","HG/T3704,阀体:WCB / PTFE Liner 阀芯:PTFE","个",6,"HQ41F46-16C DN100"]
[492,"止回阀,DN25,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:A105 阀芯:13Cr","个",16,"H41H-16C DN25"]
[493,"止回阀,DN32,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:A105 阀芯:13Cr","个",10,"H41H-16C DN32"]
[494,"止回阀,DN40,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:A105 阀芯:13Cr","个",2,"H41H-16C DN40"]
[495,"止回阀,DN20,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:F304 阀芯:304/STL","个",2,"H41Y-16P DN20"]
[496,"止回阀,DN25,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:F304 阀芯:304/STL","个",2,"H41Y-16P DN25"]
[497,"止回阀,DN32,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:F304 阀芯:304/STL","个",2,"H41Y-16P DN32"]
[498,"止回阀,DN250,PN16,RF,Dual Plate, Wafer,双板止回阀应水平安装，铰链销垂直，或垂直安装，流向向上","JB/T8937,阀体:WCB 阀芯:13Cr/STL","个",4,"H76Y-16C DN250"]
[499,"蝶阀,DN200,PN16,RF,triple offset, Gear,低泄漏性阀杆填料","GB/T12238,阀体:CF8 阀芯:304/STL","个",8,"D343Y-16P DN200"]
[500,"蝶阀,DN300,PN16,RF,triple offset, Gear,低泄漏性阀杆填料","GB/T12238,阀体:CF8 阀芯:304/STL","个",4,"D343Y-16P DN300"]
[501,"蝶阀,DN150,PN16,RF,Wafer, Gear","GB/T12238,阀体:WCB 阀芯:13Cr/EPDM","个",8,"D371X-16C DN150"]
[502,"蝶阀,DN250,PN16,RF,Gear,低泄漏性阀杆填料","GB/T12238,阀体:WCB 阀芯:13Cr/PTFE","个",8,"D341F-16C DN250"]
[503,"蝶阀,DN300,PN16,RF,Gear,低泄漏性阀杆填料","GB/T12238,阀体:WCB 阀芯:13Cr/PTFE","个",4,"D341F-16C DN300"]
[504,"蝶阀,DN150,PN16,RF,triple offset, Gear,低泄漏性阀杆填料","GB/T12238,阀体:WCB 阀芯:13Cr/STL","个",2,"D343Y-16C DN150"]
[505,"蝶阀,DN200,PN16,RF,triple offset, Gear,低泄漏性阀杆填料","GB/T12238,阀体:WCB 阀芯:13Cr/STL","个",2,"D343Y-16C DN200"]
[730,"闸阀,DN150,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","GB/T12234,阀体:CF8 阀芯:304/STL","个",18,"Z41Y-16P DN150"]
[731,"闸阀,DN50,PN16,RF,BB, OS&Y","GB/T12234,阀体:WCB 阀芯:13Cr/STL","个",30,"Z41Y-16C DN50"]
[732,"闸阀,DN80,PN16,RF,BB, OS&Y","GB/T12234,阀体:WCB 阀芯:13Cr/STL","个",15,"Z41Y-16C DN80"]
[733,"闸阀,DN32,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",12,"Z41Y-16C DN32"]
[734,"截止阀,DN50,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","GB/T12235,阀体:CF8 阀芯:304/STL","个",7,"J41Y-16P DN50"]
[735,"截止阀,DN65,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","GB/T12235,阀体:CF8 阀芯:304/STL","个",9,"J41Y-16P DN65"]
[736,"截止阀,DN50,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr","个",14,"J41H-16C DN50"]
[737,"截止阀,DN65,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr","个",8,"J41H-16C DN65"]
[738,"截止阀,DN80,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr","个",4,"J41H-16C DN80"]
[739,"截止阀,DN50,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",9,"J41Y-16C DN50"]
[740,"截止阀,DN65,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",64,"J41Y-16C DN65"]
[741,"截止阀,DN80,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",17,"J41Y-16C DN80"]
[742,"截止阀,DN125,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",24,"J41Y-16C DN125"]
[743,"截止阀,DN32,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr","个",4,"J41H-16C DN32"]
[744,"截止阀,DN25,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",2,"J41Y-16C DN25"]
[745,"截止阀,DN32,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",5,"J41Y-16C DN32"]
[746,"截止阀,DN25,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","JB/T7746,阀体:F304 阀芯:304/STL","个",6,"J41Y-16P DN25"]
[747,"截止阀,DN32,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","JB/T7746,阀体:F304 阀芯:304/STL","个",8,"J41Y-16P DN25"]
[748,"截止阀,DN40,PN16,RF,BB, OS&Y,低泄漏性阀杆填料","JB/T7746,阀体:F304 阀芯:304/STL","个",2,"J41Y-16P DN32"]
[749,"球阀,DN20,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",9,"Q41F-16P DN40"]
[750,"球阀,DN25,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",1,"Q41F-16P DN25"]
[751,"球阀,DN40,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",3,"Q41F-16P DN40"]
[752,"球阀,DN50,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",1,"Q41F-16P DN50"]
[753,"球阀,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",96,"Q41Y-16P DN20"]
[754,"球阀,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",175,"Q41Y-16P DN25"]
[755,"球阀,DN32,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",27,"Q41Y-16P DN32"]
[756,"球阀,DN40,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",12,"Q41Y-16P DN40"]
[757,"球阀,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",133,"Q41Y-16P DN50"]
[758,"球阀,DN65,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",83,"Q41Y-16P DN65"]
[759,"球阀,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",18,"Q41Y-16P DN80"]
[760,"球阀,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",8,"Q41Y-16P DN100"]
[761,"球阀,DN20,PN16,RF,Floating Ball","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",12,"Q41F-16C DN20"]
[762,"球阀,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",1,"Q41F-16C DN20"]
[763,"球阀,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",8,"Q41F-16C DN25"]
[764,"球阀,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",3,"Q41Y-16C DN50"]
[765,"球阀,DN65,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:WCB 阀芯:304/STL","个",12,"Q41Y-16C DN65"]
[766,"止回阀,DN50,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304/STL","个",18,"H44Y-16P DN50"]
[767,"止回阀,DN65,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304/STL","个",10,"H44Y-16P DN65"]
[768,"止回阀,DN50,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:WCB 阀芯:13Cr","个",12,"H44H-16C DN50"]
[769,"止回阀,DN80,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:WCB 阀芯:13Cr","个",13,"H44H-16C DN80"]
[770,"止回阀,DN25,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:A105 阀芯:13Cr","个",1,"H41H-16C DN25"]
[771,"止回阀,DN32,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:A105 阀芯:13Cr","个",4,"H41H-16C DN32"]
[772,"止回阀,DN20,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:F304 阀芯:304","个",9,"H41W-16P DN20"]
[773,"止回阀,DN25,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:F304 阀芯:304/STL","个",5,"H41Y-16P DN25"]
[774,"止回阀,DN32,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:F304 阀芯:304/STL","个",4,"H41Y-16P DN32"]
[775,"止回阀,DN40,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:F304 阀芯:304/STL","个",4,"H41Y-16P DN40"]
[776,"蝶阀,DN200,PN16,RF,triple offset, Gear,低泄漏性阀杆填料","GB/T12238,阀体:CF8 阀芯:304/STL","个",2,"D343Y-16P DN200"]
[777,"蝶阀,DN250,PN16,RF,triple offset, Gear,低泄漏性阀杆填料","GB/T12238,阀体:CF8 阀芯:304/STL","个",7,"D343Y-16P DN250"]
[778,"蝶阀,DN150,PN16,RF,Wafer, Gear","GB/T12238,阀体:WCB 阀芯:13Cr/EPDM","个",4,"D371X-16C DN150"]
[779,"蝶阀,DN300,PN16,RF,Wafer, Gear","GB/T12238,阀体:WCB 阀芯:13Cr/EPDM","个",2,"D371X-16C DN300"]
[849,"截止阀,DN50,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr","个",2,"J41H-16C DN50"]
[850,"截止阀,DN50,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",10,"J41Y-16C DN50"]
[851,"截止阀,DN25,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr","个",4,"J41H-16C DN25"]
[852,"截止阀,DN25,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",16,"J41Y-16C DN25"]
[853,"截止阀,DN25,PN16,RF,BB, OS&Y","JB/T7746,阀体:F304 阀芯:304","个",3,"J41W-16P DN25"]
[854,"球阀加长阀杆,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",6,"Q41Y-16P DN100"]
[855,"球阀加长阀杆,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",6,"Q41Y-16P DN25"]
[856,"球阀,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",8,"Q41F-16C DN25"]
[857,"球阀加长阀杆,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",12,"Q41F-16C DN25"]
[858,"球阀,DN65,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",4,"Q41F-16C DN65"]
[859,"球阀,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",11,"Q41F-16C DN80"]
[860,"球阀加长阀杆,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",2,"Q41F-16C DN80"]
[861,"球阀,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",10,"Q41F-16C DN100"]
[862,"止回阀,DN100,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304/STL","个",2,"H44Y-16P DN100"]
[863,"止回阀,DN80,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:WCB 阀芯:13Cr","个",2,"H44H-16C DN80"]
[1065,"截止阀,DN50,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",135,"J41Y-16C DN50"]
[1066,"截止阀,DN65,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",1,"J41Y-16C DN65"]
[1067,"截止阀,DN80,PN16,RF,BB, OS&Y","GB/T12235,阀体:WCB 阀芯:13Cr/STL","个",2,"J41Y-16C DN80"]
[1068,"截止阀,DN15,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",24,"J41Y-16C DN15"]
[1069,"截止阀,DN25,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",43,"J41Y-16C DN25"]
[1070,"截止阀,DN32,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",1,"J41Y-16C DN32"]
[1071,"截止阀,DN40,PN16,RF,BB, OS&Y","JB/T7746,阀体:A105 阀芯:13Cr/STL","个",2,"J41Y-16C DN40"]
[1072,"球阀加长阀杆,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:CF3M 阀芯:316L/PTFE","个",5,"Q41F-16RL DN25"]
[1073,"球阀,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:CF3M 阀芯:316L/PTFE","个",6,"Q41F-16RL DN80"]
[1074,"球阀加长阀杆,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:CF3M 阀芯:316L/PTFE","个",6,"Q41F-16RL DN80"]
[1075,"球阀,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:CF3M 阀芯:316L/PTFE","个",6,"Q41F-16RL DN100"]
[1076,"球阀加长阀杆,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:CF3M 阀芯:316L/PTFE","个",1,"Q41F-16RL DN100"]
[1077,"球阀,DN20,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",13,"Q41F-16P DN20"]
[1078,"球阀,DN25,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",4,"Q41F-16P DN25"]
[1079,"球阀,DN32,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",1,"Q41F-16P DN32"]
[1080,"球阀,DN40,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",4,"Q41F-16P DN40"]
[1081,"球阀,DN50,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",6,"Q41F-16P DN50"]
[1082,"球阀,DN65,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",1,"Q41F-16P DN65"]
[1083,"球阀,DN80,PN16,RF,Floating Ball","GB/T12237,阀体:CF8 阀芯:304/PTFE","个",3,"Q41F-16P DN80"]
[1084,"球阀,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",6,"Q41Y-16P DN25"]
[1085,"球阀加长阀杆,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",21,"Q41Y-16P DN25"]
[1086,"球阀加长阀杆,DN40,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",3,"Q41Y-16P DN40"]
[1087,"球阀,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",8,"Q41Y-16P DN50"]
[1088,"球阀加长阀杆,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",4,"Q41Y-16P DN50"]
[1089,"球阀加长阀杆,DN65,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",19,"Q41Y-16P DN65"]
[1090,"球阀,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",28,"Q41Y-16P DN80"]
[1091,"球阀,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",56,"Q41Y-16P DN100"]
[1092,"球阀加长阀杆,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料","GB/T12237,阀体:CF8 阀芯:304/STL","个",19,"Q41Y-16P DN100"]
[1093,"球阀加长阀杆,DN20,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",1,"Q41F-16C DN20"]
[1094,"球阀,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",2,"Q41F-16C DN25"]
[1095,"球阀加长阀杆,DN25,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",17,"Q41F-16C DN25"]
[1096,"球阀,DN32,PN16,RF,Floating Ball","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",1,"Q41F-16C DN32"]
[1097,"球阀,DN50,PN16,RF,Floating Ball","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",5,"Q41F-16C DN50"]
[1098,"球阀加长阀杆,DN50,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",1,"Q41F-16C DN50"]
[1099,"球阀加长阀杆,DN65,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",4,"Q41F-16C DN65"]
[1100,"球阀,DN80,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",9,"Q41F-16C DN80"]
[1101,"球阀,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",9,"Q41F-16C DN100"]
[1102,"球阀加长阀杆,DN100,PN16,RF,Floating Ball,低泄漏性阀杆填料，防火、防静电设计","GB/T12237,阀体:WCB 阀芯:304/PTFE","个",49,"Q41F-16C DN100"]
[1103,"球阀,DN25,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",5,"Q41F46-16C DN25"]
[1104,"球阀,DN50,PN16,RF,Floating Ball, Lined,低泄漏性阀杆填料","HG/T3704,阀体:WCB / PTFE Liner 阀芯:CS + PTFE","个",7,"Q41F46-16C DN50"]
[1105,"球阀,DN50,PN10,BW,True Union Ball Valve（Butt Welding Type）","Manufacturer STD,阀体:PP 阀芯:PP","个",1,"Q41S-10 DN50"]
[1106,"止回阀",null,null,{"$f":"SUBTOTAL(9,E7:E213)","v":3712}]
[1107,"止回阀,DN100,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF3M 阀芯:316L/STL","个",1,"H44Y-16RL DN100"]
[1108,"止回阀,DN65,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304","个",1,"H44W-16P DN65"]
[1109,"止回阀,DN50,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304/STL","个",2,"H44Y-16P DN50"]
[1110,"止回阀,DN65,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304/STL","个",3,"H44Y-16P DN65"]
[1111,"止回阀,DN100,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:CF8 阀芯:304/STL","个",2,"H44Y-16P DN100"]
[1112,"止回阀,DN100,PN16,RF,Swing,旋启式止回阀应水平安装，阀盖朝上，或垂直安装，流向向上","GB/T12236,阀体:WCB 阀芯:13Cr","个",12,"H44H-16C DN50"]
[1113,"止回阀,DN50,PN16,RF,Ball / Lift, Lined,球型升降式式止回阀应垂直安装，流向向上","HG/T3704,阀体:WCB / PTFE Liner 阀芯:PTFE","个",2,"HQ41F46-16C DN50"]
[1114,"止回阀,DN32,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:A105 阀芯:13Cr","个",1,"H41H-16C DN32"]
[1115,"止回阀,DN20,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:F304 阀芯:304","个",9,"H41W-16P DN20"]
[1116,"止回阀,DN40,PN16,RF,Lift,升降式止回阀应水平安装，阀盖朝上","JB/T7746,阀体:F304 阀芯:304","个",1,"H41W-16P DN40"]
[125,"Y型过滤器,DN25,PN16,RF,Mesh Size XX","HG/T21637,阀体:WCB 阀芯:304 Screen","个",16,"GL41H-16C DN25"]
[506,"Y型过滤器,DN50,PN16,RF,Mesh Size XX","HG/T21637,阀体:CF8 阀芯:304 Screen","个",4,"GL41W-16P DN50"]
[507,"Y型过滤器,DN25,PN16,RF,Mesh Size XX","HG/T21637,阀体:WCB 阀芯:304 Screen","个",4,"GL41H-16C DN25"]
[508,"Y型过滤器,DN65,PN16,RF,Mesh Size XX","HG/T21637,阀体:WCB 阀芯:304 Screen","个",6,"GL41H-16C DN65"]
[509,"Y型过滤器,DN80,PN16,RF,Mesh Size XX","HG/T21637,阀体:WCB 阀芯:304 Screen","个",2,"GL41H-16C DN80"]
[780,"Y型过滤器,DN32,PN16,RF,Mesh Size XX","HG/T21637,阀体:CF8 阀芯:304 Screen","个",1,"GL41W-16P DN32"]
[781,"Y型过滤器,DN40,PN16,RF,Mesh Size XX","HG/T21637,阀体:CF8 阀芯:304 Screen","个",2,"GL41W-16P DN40"]
[782,"Y型过滤器,DN50,PN16,RF,Mesh Size XX","HG/T21637,阀体:CF8 阀芯:304 Screen","个",16,"GL41W-16P DN50"]
[783,"Y型过滤器,DN65,PN16,RF,Mesh Size XX","HG/T21637,阀体:CF8 阀芯:304 Screen","个",12,"GL41W-16P DN65"]
[784,"Y型过滤器,DN80,PN16,RF,Mesh Size XX","HG/T21637,阀体:CF8 阀芯:304 Screen","个",8,"GL41W-16P DN80"]
[864,"Y型过滤器,DN100,PN16,RF,Mesh Size XX","HG/T21637,阀体:CF8 阀芯:304 Screen","个",2,"GL41W-16P DN100"]
[865,"Y型过滤器,DN80,PN16,RF,Mesh Size XX","HG/T21637,阀体:WCB 阀芯:304 Screen","个",2,"GL41H-16C DN80"]
[1117,"Y型过滤器,DN50,PN16,RF,Mesh Size XX","HG/T21637,阀体:CF8 阀芯:304 Screen","个",3,"GL41W-16P DN50"]
[1118,"Y型过滤器,DN100,PN16,RF,Mesh Size XX","HG/T21637,阀体:CF8 阀芯:304 Screen","个",1,"GL41W-16P DN100"]
[1119,"Y型过滤器,DN40,PN16,RF,Mesh Size XX","HG/T21637,阀体:WCB 阀芯:304 Screen","个",1,"GL41H-16C DN40"]
[1120,"Y型过滤器,DN50,PN16,RF,Mesh Size XX","HG/T21637,阀体:WCB 阀芯:304 Screen","个",24,"GL41H-16C DN50"]
[1121,"Y型过滤器,DN100,PN16,RF,Mesh Size XX","HG/T21637,阀体:WCB 阀芯:304 Screen","个",1,"GL41H-16C DN100"]

{"sheet":"各个型号数量","index":1,"n_rows":99,"n_cols":17,"rows_kept":99,"merged":[[1,8,39,8],[1,9,8,9],[9,9,12,9],[13,9,19,9],[14,0,14,7],[20,9,25,9],[26,9,30,9],[30,0,30,7],[32,9,39,9],[46,0,46,8],[63,0,63,8],[81,0,81,8],[98,0,98,8]]}
["球阀","Q41F-16C","Q41F-16RL","Q41F-16P","Q41F46-16C","Q41Y-16C","Q41S-10","Q41Y-16P"]
["DN20",182,2,91,15,40,null,144]
["DN25",203,6,29,112,null,null,33]
["DN32",57,null,1,{"$nulls":3},33]
["DN40",2,{"$nulls":5},15]
["DN50",109,null,14,129,17,1,189]
["DN65",86,null,3,37,46,null,152]
["DN80",78,16,4,27,28,null,58]
["DN100",81,7,1,65,10,null,130]
["DN125"]
["DN150"]
["DN200"]
["DN250"]
["DN300"]
["备注：软密封球阀均采用防火防静电结构，球阀均为实心球，球阀标准：GB/T12237-2007，结构长度：JB/1686，法兰标准和等级：HG/T20592-2009 PN16 RF,壁厚达标件"]
["截止阀","J41Y-16C ","J41H-16C","J41W-16P","J41Y-16C","J41Y-16P"]
["DN15",{"$nulls":3},24]
["DN20",64,null,null,64]
["DN25",137,34,3,137,14]
["DN32",93,14,null,93,2]
["DN40",8,null,null,8]
["DN50",248,50,1,248,7]
["DN65",65,null,null,65,11]
["DN80",31,null,null,31]
["DN100"]
["DN125",null,4,null,24]
["DN150",null,4,null,2]
["DN200"]
["DN250"]
["DN300"]
["备注：GB/T12235-2007,法兰标准和等级：HG/T20592-2009 PN16 RF"]
["闸阀","Z41Y-16C","Z41Y-16P"]
["DN15"]
["DN20",56]
["DN25",1]
["DN32",13]
["DN40"]
["DN50",37]
["DN65",8]
["DN80",15]
["DN100"]
["DN125"]
["DN150",18,18]
["DN200",1]
["DN250"]
["DN300"]
["备注:GB/T12234-2007,法兰标准和等级：HG/T20592-2009 PN16 RF"]
["止回阀","H76H-16C","H44Y-16RL","H44W-16P","H44H-16C","H44F46-16C","HQ41F46-16C","H41H-16C","H41Y-16P","H76Y-16C","H44Y-16P ","H44H-16C","H41H-16C","H41W-16P","H41Y-16P","H44Y-16P","H44W-16P "]
["DN15"]
["DN20",{"$nulls":7},2,{"$nulls":4},18,2]
["DN25",{"$nulls":5},6,17,7,{"$nulls":3},17,null,7]
["DN32",{"$nulls":6},15,6,{"$nulls":3},15,null,6]
["DN40",{"$nulls":6},2,4,{"$nulls":3},2,1,4]
["DN50",null,null,2,34,null,21,{"$nulls":3},24,34,{"$nulls":3},24,2]
["DN65",null,null,1,22,null,9,{"$nulls":3},15,22,{"$nulls":3},15,1]
["DN80",null,1,null,24,{"$nulls":6},24,{"$nulls":3},15]
["DN100",null,1,{"$nulls":3},6,{"$nulls":3},4]
["DN125",{"$nulls":4},8,{"$nulls":9},4]
["DN150"]
["DN200"]
["DN250",{"$nulls":8},4]
["DN300"]
["DN350",5]
["备注:GB/T12235-2007,法兰标准和等级：HG/T20592-2009 PN16 RF"]
[]
["蝶阀","D371X-16C ","D343Y-16P ","D341F-16C ","D343Y-16C "]
["DN15"]
["DN20"]
["DN25"]
["DN32"]
["DN40"]
["DN50"]
["DN65"]
["DN80"]
["DN100"]
["DN125"]
["DN150",12,null,null,2]
["DN200",null,10,null,2]
["DN250",null,7,8]
["DN300",2,4,4,2]
["DN350",10]
["备注：GB/T12238-2008,法兰标准和等级：HG/T20592-2009 PN16 RF"]
["Y型过滤器","GL41H-16C","GL41W-16P "]
["DN15"]
["DN20"]
["DN25",20]
["DN32",null,1]
["DN40",1,2]
["DN50",24,23]
["DN65",6,12]
["DN80",4]
["DN100",1,3]
["DN125"]
["DN150"]
["DN200"]
["DN250"]
["DN300"]
["DN350"]
["备注: HG/T 21637-2021 ,法兰标准和等级：HG/T20592-2009 PN16 RF"]

{"sheet":"Sheet2","index":2,"n_rows":140,"n_cols":5,"rows_kept":140,"merged":[[1,1,39,1],[1,2,8,2],[9,2,12,2],[13,2,19,2],[20,2,25,2],[26,2,30,2],[32,2,39,2],[40,1,67,1],[40,2,46,2],[47,2,51,2],[52,2,53,2],[54,2,63,2],[64,2,67,2],[68,1,76,1],[68,2,75,2],[77,1,117,1],[78,2,79,2],[80,2,81,2],[82,2,84,2],[86,2,89,2],[90,2,92,2],[93,2,96,2],[98,2,100,2],[101,2,103,2],[104,2,106,2],[107,2,108,2],[109,2,112,2],[113,2,115,2],[116,2,117,2],[118,1,128,1],[118,2,120,2],[121,2,123,2],[124,2,125,2],[126,2,128,2],[129,1,139,1],[129,2,134,2],[135,2,139,2]]}
["序号","类别","型号","口径","数量"]
[1,"球阀\n(软密封球阀均采用防火防静电结构，球阀均为实心球，球阀标准：GB/T12237-2007，结构长度：JB/1686，法兰标准和等级：HG/T20592-2009 PN16 RF,壁厚达标件)","Q41F-16C","DN20",182]
[2,null,null,"DN25",203]
[3,null,null,"DN32",57]
[4,null,null,"DN40",2]
[5,null,null,"DN50",109]
[6,null,null,"DN65",86]
[7,null,null,"DN80",78]
[8,null,null,"DN100",81]
[9,null,"Q41F-16RL","DN20",2]
[10,null,null,"DN25",6]
[11,null,null,"DN80",16]
[12,null,null,"DN100",7]
[13,null,"Q41F-16P","DN20",91]
[14,null,null,"DN25",29]
[15,null,null,"DN32",1]
[16,null,null,"DN50",14]
[17,null,null,"DN65",3]
[18,null,null,"DN80",4]
[19,null,null,"DN100",1]
[20,null,"Q41F46-16C","DN20",15]
[21,null,null,"DN25",112]
[22,null,null,"DN50",129]
[23,null,null,"DN65",37]
[24,null,null,"DN80",27]
[25,null,null,"DN100",65]
[26,null,"Q41Y-16C","DN20",40]
[27,null,null,"DN50",17]
[28,null,null,"DN65",46]
[29,null,null,"DN80",28]
[30,null,null,"DN100",10]
[31,null,"Q41S-10","DN50",1]
[32,null,"Q41Y-16P","DN20",144]
[33,null,null,"DN25",33]
[34,null,null,"DN32",33]
[35,null,null,"DN40",15]
[36,null,null,"DN50",189]
[37,null,null,"DN65",152]
[38,null,null,"DN80",58]
[39,null,null,"DN100",130]
[40,"截止阀\n(GB/T12235-2007,法兰标准和等级：HG/T20592-2009 PN16 RF)","J41Y-16C ","DN20",64]
[41,null,null,"DN25",137]
[42,null,null,"DN32",93]
[43,null,null,"DN40",8]
[44,null,null,"DN50",248]
[45,null,null,"DN65",65]
[46,null,null,"DN80",31]
[47,null,"J41H-16C","DN25",34]
[48,null,null,"DN32",14]
[49,null,null,"DN50",50]
[50,null,null,"DN125",4]
[51,null,null,"DN150",4]
[52,null,"J41W-16P","DN25",3]
[53,null,null,"DN50",1]
[54,null,"J41Y-16C","DN15",24]
[55,null,null,"DN20",64]
[56,null,null,"DN25",137]
[57,null,null,"DN32",93]
[58,null,null,"DN40",8]
[59,null,null,"DN50",248]
[60,null,null,"DN65",65]
[61,null,null,"DN80",31]
[62,null,null,"DN125",24]
[63,null,null,"DN150",2]
[64,null,"J41Y-16P","DN25",14]
[65,null,null,"DN32",2]
[66,null,null,"DN50",7]
[67,null,null,"DN65",11]
[68,"闸阀\n(GB/T12234-2007,法兰标准和等级：HG/T20592-2009 PN16 RF)","Z41Y-16C","DN20",56]
[69,null,null,"DN25",1]
[70,null,null,"DN32",13]
[71,null,null,"DN50",37]
[72,null,null,"DN65",8]
[73,null,null,"DN80",15]
[74,null,null,"DN150",18]
[75,null,null,"DN200",1]
[76,null,"Z41Y-16P","DN150",18]
[77,"止回阀\n(GB/T12235-2007,法兰标准和等级：HG/T20592-2009 PN16 RF)","H76H-16C","DN350",5]
[78,null,"H44Y-16RL","DN80",1]
[79,null,null,"DN100",1]
[80,null,"H44W-16P","DN50",2]
[81,null,null,"DN65",1]
[82,null,"H44H-16C","DN50",34]
[83,null,null,"DN65",22]
[84,null,null,"DN80",24]
[85,null,"H44F46-16C","DN125",8]
[86,null,"HQ41F46-16C","DN25",6]
[87,null,null,"DN50",21]
[88,null,null,"DN65",9]
[89,null,null,"DN100",6]
[90,null,"H41H-16C","DN25",17]
[91,null,null,"DN32",15]
[92,null,null,"DN40",2]
[93,null,"H41Y-16P","DN20",2]
[94,null,null,"DN25",7]
[95,null,null,"DN32",6]
[96,null,null,"DN40",4]
[97,null,"H76Y-16C","DN250",4]
[98,null,"H44Y-16P ","DN50",24]
[99,null,null,"DN65",15]
[100,null,null,"DN100",4]
[101,null,"H44H-16C","DN50",34]
[102,null,null,"DN65",22]
[103,null,null,"DN80",24]
[104,null,"H41H-16C","DN25",17]
[105,null,null,"DN32",15]
[106,null,null,"DN40",2]
[107,null,"H41W-16P","DN20",18]
[108,null,null,"DN40",1]
[109,null,"H41Y-16P","DN20",2]
[110,null,null,"DN25",7]
[111,null,null,"DN32",6]
[112,null,null,"DN40",4]
[113,null,"H44Y-16P","DN50",24]
[114,null,null,"DN65",15]
[115,null,null,"DN80",15]
[116,null,"H44W-16P ","DN50",2]
[117,null,null,"DN65",1]
[118,"蝶阀\n(GB/T12238-2008,法兰标准和等级：HG/T20592-2009 PN16 RF)","D371X-16C ","DN150",12]
[119,null,null,"DN300",2]
[120,null,null,"DN350",10]
[121,null,"D343Y-16P ","DN200",10]
[122,null,null,"DN250",7]
[123,null,null,"DN300",4]
[124,null,"D341F-16C ","DN250",8]
[125,null,null,"DN300",4]
[126,null,"D343Y-16C ","DN150",2]
[127,null,null,"DN200",2]
[128,null,null,"DN300",2]
[129,"Y型过滤器\n(HG/T 21637-2021 ,法兰标准和等级：HG/T20592-2009 PN16 RF)","GL41H-16C","DN25",20]
[130,null,null,"DN40",1]
[131,null,null,"DN50",24]
[132,null,null,"DN65",6]
[133,null,null,"DN80",4]
[134,null,null,"DN100",1]
[135,null,"GL41W-16P ","DN32",1]
[136,null,null,"DN40",2]
[137,null,null,"DN50",23]
[138,null,null,"DN65",12]
[139,null,null,"DN100",3]